Air FX
by Aerie kites

Wingspan			2380			all measurements are in mm

Height			1190 / 1020 		standing / keel

Spars
upper spreader		.220 		x 502 / 540	
lower spreder			G-Force ul 	x 825
spine				.230 		x 1000
leading edge	upper		G-Force ul 	x 825
		lower		G-Force ul 	x 825	

Distances			(middle of the nosetip to middle of the connector)
nose - us			340			
nose - ls			1130			
nose - cross			722			

end of the nock - ls		555
us - ls				790

Standoff			
inner	2,5 mm CFK		207			
distance from cross		330
outer				308	
(measured from the middle of the cross to the middle of the connector)

Bridle 			(measured on the kite)
us - x 				655		
ls - x				695			
cross - x			685			

Weight			
brutto	(gr.)			263