Araneus
by Spiderkites

Wingspan			2340			all measurements are in mm	 

Height			1000 /	910		standing / keel			

Spars
upper spreader		6mm	 x 520
lower spreader		DT15	 x 732
spine				T15	 x 890
leading edge	upper		D12	 x 750	
		lower		D12	 x 750	

Distances			(middle of the nosetip to middle of the connector)
nose - us			335			
us - ls				620
us - yoyo stopper		230
nose - cross			

Standoff			
inner				252		
distance from cross		230			
outer				252			
distance from cross		355			
(measured from the middle of the cross to the middle of the connector)

Bridle 			(measured on the kite)
us - x 				550		
ls - x				570			
cross - x			560			
us knots			20, 40, 60
optional inverse turbo	20 and 60

Weights			
keel	(gr.)			15,5

Weight
brutto	(gr.)			282	

Wingtips have 6mm inserts, so the nocks are flush.
Bridlepoints: oQs - upper, uQs - lower, keel - 7 cm under
Bridle with inverse turbo option