Duende 2.4 std.
by Flying Wings

Wingspan			2400			all measurements are in mm

Height			970 / 950		standing / keel	

Spars
upper spreader		6mm x 525
lower spreader		DT12 x 711
spine				DT12 x 760, 		plus 6mm x 165/200 extension
leading edge	upper		DT12 x 760
		lower		DT12 x 760	

Distances			(middle of the nosetip to middle of the connector)
nose - us			355			
nose - ls			930			
nose - yoyo stopper		585
nose - cross			595			

Standoff	
Inner	3 mm CFK		275		
distance from cross		240			
outer 	3mm CFK		280			
distance from cross		305	
(measured from the middle of the cross to the middle of the connector)

Bridle
us - x 				530		
ls - x				450			
cross - x			570			
Turbo				62

Weights			
Kiel	(gr.)			20

Weight
brutto	(gr.)			311

bridleknot directly above the us connector, 
20mm below the ls connector and  
20 mm below the cross