Eternity std.
by Level One

Wingspan			2320			all measurements are in mm

Height			950 / 910		standing / keel

Spars
upper spreader		 5,5		x 520	
lower spreder			 PT5		x 7305
spine				 PT5		x 890	thin tip (cut) on top
leading edge	upper		 P100		x 660
		lower		 P100		x 825	

Distances			(middle of the nosetip to middle of the connector)
nose - us			340			
us - ls				595			
us - yoyo stopper		200
nose - cross			600		

Standoff			
inner	3 mm CFK		260			
distance from cross		300
outer	3 mm CFK		270
distance from cross		355
(measured from the middle of the cross to the middle of the connector)

Bridle 			(measured on the kite)
us - x 				530
ls - x				480			
cross - x			570			

Weights			
keel	(gr.)			10

Weight			
brutto	(gr.)			285