Fluid ul

Wingspan			2480			all measurements are in mm

Height			980 / 950		standing / keel

Spars
upper spreader		 5		x 565	
lower spreder			 BD PT3	x 825
spine				 D20		x 945	thin tip (cut) on top
leading edge	upper		 PT3		x 725
		lower		 P100		x 825	

Distances			(middle of the nosetip to middle of the connector)
nose - us			375			
us - ls				685			
us - yoyo stopper		230
nose - cross			630		

Standoff			
inner	3 mm CFK		255			
distance from cross		205
outer	3 mm CFK		265
distance from cross		310
(measured from the middle of the cross to the middle of the connector)

Bridle 			(measured on the kite) - experimental !!!
us - x 				560
ls - x				540			
cross - x			670			

Weights			
keel	(gr.)			20

Weight			
brutto	(gr.)			303	

This is my version of it, made with a std. sail. Highly experimental.
Shape 2
low LevelOne Kenny-cross, 
4x big APA's, 
sail standoff connectors by LevelOne with screws
Weight glued in a rubber cap
my le is just 1500 mm - perhaps a bit to short