Ice - tuned

Wingspan			1530			all measurements are in mm

Height			545 / 455		standing / keel

Spars
upper spreader		 5		x 368	
lower spreder			 6		x 564
spine				 5		x 450
leading edge			 5		x 910

Distances			(middle of the nosetip to middle of the connector)
nose - us			220			
us - ls				465			
us - yoyo stopper		
nose - cross			356		

Standoff			
outer	3 mm GFK wound	138
distance from cross		402
(measured from the middle of the cross to the middle of the connector)

Bridle 			(measured on the kite)
us - x 				450
ls - x				480			
cross - x			505			

Weights			
keel	(gr.)			

Weight			
brutto	(gr.)			

Tuning:
- glitter application off
- all tubes sanded at the ends!
- le tensioning changed from rubber band to string
- standoffs changed to 3 mm wound GFK (black!)