Jumping Jack Flash std.
by Level One

Wingspan			2060			all measurements are in mm

Height			930 / 835		standing / keel

Spars
upper spreader		6		x 505	
lower spreader		P200		x 690
spine				P300		x 825
leading edge			5,5		x 1370	

Distances			(middle of the nosetip to middle of the connector)
nose - us			320			
us - ls				680			
us - yoyo stopper		200
nose - cross			570		

Standoff			
inner	3 mm CFK		260			
distance from cross		195
outer	3 mm GFK		255			
distance from cross		315
(measured from the middle of the cross to the middle of the connector)

Bridle - super cross	(measured on the kite)
us - x 				490
ls - x				490			
cross - x			540

Weights			
keel	(gr.)			6

Weight			
brutto	(gr.)			280